1. V1.13 for LT165 256Mbits(32bits address) norflash 
2. V1.20B for the size of bin over 1Mbytes to download to the spiflash of the programmer board 
3. V1.20C support LT779 NandFlash program with "LT_Programmer_APP_withCDC_V1.25.app"